**Annex 3. Conditions for Packaging and Delivering Spare Parts**

1. **Labelling Spare Parts (hereinafter „Goods“)**

The label attached to the original packaging of the Goods must contain the following details at a minimum:

* name of the Goods;
* vehicle make;
* NSN-code (if applicable);
* product code;
* the Seller’s warehouse code.

1. **Packaging**

When transporting Goods on pallets, the products are packaged into grouped packaging (packing crates). The Seller agrees to provide packaging that ensures the Goods’ conservation during its transportation to the destination and its long-term storage in unchanged form.

Labels for grouped packaging are at least an A4-size in capital letters and in bold. The minimum letter height is 8 mm. There is a label on at least two sides of the packing box.

The labelling details on the label are in the following order:

* name of the Goods;
* product and/or NSN-code (if applicable);
* quantity and unit (pieces/EA);
* delivery time (month and year);
* contract number and batch number (if the Goods are delivered in several parts);
* the Seller’s name;
* the Seller’s address;
* delivery address.

Packing crates are placed on pallets. The pallet dimensions are 800x1200 mm. Pallets must be intact (not decayed, mouldy and with no broken boards), clean and there cannot be any protruding nails. Pallets must endure the long-term storage of the Goods. The maximum height of packing crates placed on pallets is 1200 mm (pallets are not returnable). Plastic film is used for transport, which covers the packing crates on the pallets. Plastic film keeps the product crates firmly on pallets and protects them from the elements.

Labels for transporting packaging are at least an A4-size in capital letters and in bold. The minimum letter height is 8 mm. There is a label attached on all sides (four labels on one package). The conservation conditions are up to five years in ventilated permanent structures. Transport is in confined form and on land, air and sea. The package must endure handling with mechanical tools. The labelling details on the label are in the following order:

* NSN-code (if applicable);
* product name;
* quantity and unit (pieces/EA);
* delivery time (month and year);
* contract number and batch number;
* the Seller’s name;
* the Seller’s address;
* delivery address.

If the order is for a single product or a small quantity of Goods, then the Goods must be packaged in other appropriate and suitable packaging. The cost of the Goods’s packaging is covered within the cost of the sold Goods.

1. **Delivery Conditions**

The Goods must be delivered unbroken and unspoiled and in suitable packaging for transport.

The Buyer shall specify delivery locations during the performance of the Contract. Transport of the Goods to the destination set by the Buyer takes place with the Seller’s own mode of transportation.