**TECHNICAL DATA SHEET**

**AB COMFORT PPI**

|  |  |  |
| --- | --- | --- |
| Kuva 1 |  |  |
| Front view | Back view | Side view |

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Description | Color | MTS / MTO |
| 1KL6C0ES1NS0 | AB COMFORT PPI MALE | BLACK | MTS |
| 1KM9C0ES1NS0 | AB COMFORT PPI FEMALE | BLACK | MTS |

**OVERVIEW**

The outer materials are light and made from high abrasion resistant polyamide with PU coating. Lining is extremely breathable 3D spacer for maximal comfort and heat dissipation. The armor cut is optimized for firearm handling and adjustable shoulder straps ensure good and comfortable fit for every user. Front and back parts have an insert plate pocket for additional protection.

**TECHNICAL DATA**

**Model details**

Panel shape AB

Available in sizes XS, S, M, L, XL, 2XL, 3XL

Protective area, L-size Front and back panel - 0,31m2

Weight, L-size around 2,6 kg, depending on ballistic panels

Cover material PU coated polyamide

Lining material Polyester 3D spacer (COOLMAX®)

Colors Black

Additional modules Insert plate, Carrying bag