Solid colors:

Acrylic acid Polymers, Xylene (mixture of isomers), Mesitylene, Cumene, Kiwoprint TC2500/1, Bisrhenola type epoxy resin, 1,4-Xylene, 2-Ethoxyethyl Acetate, Polyethylene Glycol terephthalate, Ethylene Glycol Monobutyl Ether, 1,3 Styrene block copolymer, Polyethylene glycol 200 diacrylate, Polyurethane acrylate, #520 transparent ink, Bayhydur XP, Auxiliares, TPO2.4.6, 4-(2,6,6-Trimethyl-1Cyclohexen-1-y1)-3-Buten-2-One, UNIPURE white LC 981, UNIPURE black LC 989, UNIPURE blue LC 680, UNIPURE red LC 3079, UNIPURE red LC 327,, UNIPURE yellow LC 124, UNIPURE yellow LC 125.

Glitter:

Acrylic acid Polymers, Xylene (mixture of isomers), Mesitylene, Cumene, Kiwoprint TC2500/1, Bisrhenola type epoxy resin, 1,4-Xylene, 2-Ethoxyethyl Acetate, Polyethylene Glycol terephthalate, Ethylene Glycol Monobutyl Ether, 1,3 Styrene block copolymer, Polyethylene glycol 200 diacrylate, Polyurethane acrylate, #520 transparent ink, Bayhydur XP, Auxiliares, TPO2.4.6, 4-(2,6,6-Trimethyl-1Cyclohexen-1-y1)-3-Buten-2-One, UNIPURE white LC 981, UNIPURE black LC 989, UNIPURE blue LC 680, UNIPURE red LC 3079, UNIPURE red LC 327,, UNIPURE yellow LC 124, UNIPURE yellow LC 125, PET, Aluminium or Zinc Sulfide.

Metallic gold:

Acrylic acid Polymers, Xylene (mixture of isomers), Mesitylene, Cumene, Kiwoprint TC2500/1, Bisrhenola type epoxy resin, 1,4-Xylene, 2-Ethoxyethyl Acetate, Polyethylene Glycol terephthalate, Ethylene Glycol Monobutyl Ether, 1,3 Styrene block copolymer, Polyethylene glycol 200 diacrylate, Polyurethane acrylate, #520 transparent ink, Bayhydur XP, Auxiliares, TPO2.4.6, 4-(2,6,6-Trimethyl-1Cyclohexen-1-y1)-3-Buten-2-One, UNIPURE white LC 981, UNIPURE black LC 989, UNIPURE blue LC 680, UNIPURE red LC 3079, UNIPURE red LC 327,, UNIPURE yellow LC 124, UNIPURE yellow LC 125, Quartz (SiO2), Polyethylene Terephtalate, Polyurethane, Gold Flake, Poly(ethylene-co-vinylacetate), Polypropylene, Chlorinated, Polyethylene, Mixed Resin, Ethyl Acetate, Isopropy Alcohol.