|  |  |
| --- | --- |
| **Lisa 2** – **Hoone ja Ruumide tehnilised ja ehituslikud lahendused**   1. Hoone tehniline kirjeldus vastab dokumendile: TARTU HONDA MÜÜGIESINDUS. AS RTG PROJEKTBÜROO töö nr 03/2012 20.05.2013 2. Valgustus – madala tarbimisega LED valgustus. Teeninduses 1000 lx töötasapinnal. 3. Elekter – liitumislepingu amprid mitte vähem kui 200A. 4. Seinad, põrandad ja laed on sanitaarremonditud ja puhtad. 5. Siseseintelt ja fassaadilt on eemaldatud kõik eelmise üürniku esindatavatele brändidele viitavad elemendid. | **Annex 2** – **Technical and constructional solution of the Building and the Premises**   1. The technical description of the building corresponds to the document: TARTU HONDA MÜÜGIESINDUS. AS RTG PROJEKTBÜROO töö nr 03/2012 20.05.2013 2. Lighting - low consumption LED lighting. In service area - 1000 lx above working surface. 3. Electricity - amperes of the connection agreement not less than 200A. 4. Walls, floors and ceilings are clean and have undergone sanitary repairs. 5. All elements referring to the brands represented by the previous lessee have been removed from the interior walls and facade. |